3. Write an assembly language program for adding two 16-bit data using 8086 processor.

LDA 2050

MOV B,A

LDA 2052

ADD B

STA 2053

MOV B,A

LDA 2059

ADC B

STA 2060

HLT

